Open topic with navigation

# GetStatus

The `GetStatus` action is used to get information about the current state of HPE CFS. `GetStatus` is a synchronous action. It takes no parameters and returns the following values:

Value | Description
--- | ---
product | The name of the product.
version | The product version.
build | The product build.
aciport | The ACI port used by HPE CFS.
serviceport | The service port used by HPE CFS.
directory | The running directory.
acithreads | The number of threads configured for ACI commands.
ingest | The attributes in the ingest tag count the number of requests made to CFS. `Calls` is the total number of requests. `Adds` is the total number of add requests. `Updates` is the total number of update requests. `Removes` is the total number of remove requests.
nodes | The number of documents waiting to be collected into an index batch (the number of documents that HPE CFS has finished importing).
importactive | The number of documents currently being imported.
importpending | The number of documents waiting to be imported.
keyviewmemory | The amount of memory allocated to the KeyView process.
import | Details about the number of documents imported. The `import` tag contains the following attributes: `Queued` is the number of documents that were added to the import queue. `Started` is the number of documents that started the import process. `Finished` is the number of documents that were imported successfully. `Cancelled` is the total number of documents that were canceled during the import process. Documents are canceled if you use a Pre or Post import task to run a Lua script, and the script returns `false`.

NOTE:

`GetStatus` is an administrative action that you can send only from HPE Connector Framework Server AdminClients (which you set in the HPE Connector Framework Server configuration file `[Server]` section).

## Example

    http://12.3.4.56:7000/action=GetStatus

This action uses port `7000` to request details about HPE Connector Framework Server, which is located on a machine with the IP address `12.3.4.56`.

## Response

The following XML is a sample response from the `GetStatus` action:

    <autnresponse>
       <action>GETSTATUS</action>
       <response>SUCCESS</response>
       <responsedata>
          <product>Connector Framework</product>
          <version>7.6.0.0</version>
          <build>1</build>
          <aciport>7000</aciport>
          <serviceport>7532</serviceport>
          <directory>C:\ConnectorFramework</directory>
          <acithreads>4</acithreads>
          <ingest calls="1" adds="1"/>
          <nodes>2</nodes>
          <importactive>0</importactive>
          <importpending>0</importpending>
          <keyviewmemory>0</keyviewmemory>
          <import queued="2" started="2" finished="2"/>
       </responsedata>
    </autnresponse>

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm