Open topic with navigation

# TimeoutMS

The time in milliseconds after which HPE Coordinator stops trying to collect statistics if there is no response from the HPE Controller.

Type: | String
Default: | 30000
Required: | Yes
Configuration Section: | StatsCollector and Connection If you set this parameter in the StatsCollector and Connection sections, the setting in the StatsCollector section takes precedence for statistics collection.
Example: | `Retries=1`
See Also: |

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm