Open topic with navigation

# ControllerUUIDs

A comma-separated list of HPE Controller UUIDs. Each HPE Controller has a UUID (Universal Unique ID) that consists of a 36-byte string representing a 128-bit ID. You must specify the UUID of the HPE Controller you want to return statistics for by using SSDP (SImple Service Discovery Protocol).

Actions: | GetStatistics
Type: | String
Default: | None
Required: | No
Example: | `ControllerUUIDs=d267cf80-063a-8030-a2de-24be0523821c,de262vg90-152p-7540-g2de-24be0529821c`
See Also: |

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm