Open topic with navigation

# RequireGSSAuth

Set `RequireGSSAuth` to `True` to enable GSSAPI authentication mode on the HPE Content Component index port. In this mode, all connections to the index port must be authenticated using GSSAPI and the Negotiate HTTP authentication mechanism.

To use GSSAPI authentication, you must also set GSSServiceName in the `[Server]` section, to define the GSSAPI service name that HPE Content Component must use to identify itself.

NOTE:

This method provides an authentication requirement only. HPE recommends that you use it in conjunction with TLS/SSL to encrypt the authentication data.

Type: | Boolean
Default: | False
Required: | No
Configuration Section: | IndexServer
Example: | `RequireGSSAuth=True`
See Also: | GSSServiceName

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm