Open topic with navigation

# TermCachePersistentMinOccs

The minimum number of times that a term must occur in the index for HPE Content Component to store it in the term cache in memory.The default value is `0` (zero), which means that HPE Content Component does not cache terms.

If you set both `TermCachePersistentMinOccs` and TermCachePersistentKB, TermCachePersistentKB takes precedence.

Type: | Long
Default: | 0
Allowed Range: | Minimum: 0 Maximum: 1024000
Recommended Range: | Minimum: 10240 Maximum: 1024000
Required: | No
Configuration Section: | TermCache
Example: | `TermCachePersistentMinOccs=2000000`
See Also: | TermCachePersistentKB

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm