Open topic with navigation

# Interval

After HPE Controller has collected new statistics, it compresses old data for each compression level by taking all intervals of the length specified by the `Interval` configuration parameter, and replacing them with an average or sample value.

HPE Controller begins compression at the point where statistics have a timestamp that is divisible by the value of the `Interval` configuration parameter. An average value is used for compression of numerical statistics. For other statistics, HPE Controller uses the most frequent value in the statistics for compression.

If you set `Interval` to `0`, HPE Controller removes statistics that are older than the value of `MinAge`, rather than compressing them.

For clarity, HPE recommends that you specify the name of the level that deletes statistics as `ThrowAway`, rather than `CompressLevelN`.

Type: | Long
Default: | None
Required: | Yes
Configuration Section: | CompressLevelN
Example: | `Interval=120`
See Also: | Levels MinAge

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm