Open topic with navigation

# Levels

The number of compression levels to apply to old statistical data.

The `StatsCompression` section of the configuration file must also include a line for each of the levels you specify, numbered consecutively and starting from 0 (zero).

For example, if you set `Levels` to `2`, you should include the following lines:

    0=CompressLevel0
    1=CompressLevel1

You must then add separate sections in the configuration file, `[CompressLevel0]` and `[CompressLevel1]`, where you can specify the details of the compression for each level.

For clarity, HPE recommends that you specify the name of the level that deletes statistics as `ThrowAway`, rather than `CompressLevelN`.

NOTE:

If you use a shared statistics database for HPE Coordinator and HPE Controller components, you must not configure statistics compression in both the Coordinator and HPE Controller configuration files.

For consistency, when you use a shared statistics database, HPE recommends that you configure statistics compression only in the HPE Controller components.

Type: | Integer
Default: | None
Required: | Yes
Configuration Section: | StatsCompression
Example: | `Levels=3`
See Also: |

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm