Open topic with navigation

# CommsEncryptionType

The encryption type for returned data.

In general, HPE recommends configuring Secure Socket Layer (SSL) connections between ACI servers and applications, instead of using ACI encryption. For more information, see Secure Socket Layer Parameters.

If you configure HPE Controller as part of a system that uses the Kerberos protocol for communication, set `CommsEncryptionType` to `GSS`.

To use this option, you must have a suitable library to provide the GSSAPI. On Linux systems, you might also need to create a symbolic link for the GSSAPI library to `gssapi32.so` in the working directory of the component.

Type: | String
Default: |
Required: | No
Configuration Section: | ACIEncryption
Example: | `CommsEncryptionType=GSS`
See Also: | CommsAllowUnencrypted ServiceName

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm