Open topic with navigation

# Statistics Compression Configuration Parameters

This section describes the `StatsCompression` configuration settings that control how HPE Controller compresses old statistical data.

NOTE:

If you use a shared statistics database for HPE Coordinator and HPE Controller components, you must not configure statistics compression in both the Coordinator and HPE Controller configuration files.

For consistency, when you use a shared statistics database, HPE recommends that you configure statistics compression only in the HPE Controller components.

For example:

    [StatsCompression]
    Levels=3
    0=CompressLevel0
    1=CompressLevel1
    2=ThrowAway

    [CompressLevel0]
    MinAge=3600
    Interval=120

    [CcompressLevel1]
    MinAge=86400
    Interval=3600

    [ThrowAway]
    MinAge=2592000
    Interval=0

Interval
Levels
MinAge

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm