Open topic with navigation

# UUID

The UUID of the Controller that you want to register with Coordinator.

Each Controller has a UUID (Universal Unique ID), which is a 36-byte string that represents a 128-bit ID.

NOTE:

You can register Controllers by UUID only if you enable SSDP in your Controllers. In this case, you can use the GetControllers action to obtain the UUID of a Controller.

Actions: | AddController
Type: | String
Default: | None
Required: | No
Example: | `UUID=d267cf80-063a-8030-a2de-24be0523821c`
See Also: | SSDP Configuration Parameters

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm