# VMS Ingest Engine

The VMS ingest engine ingests video streamed from a Micro Focus Video Management Server.

Configuration Parameter | Description
--- | ---
StreamTimeout | The maximum amount of time to wait for the next frame.
Type | The type of ingest engine to use. Set this parameter to `VMS`.

The VMS ingest engine produces the following tracks, where `taskName` is the name of the ingest task:

- `taskName.Image_1` - an image track that contains the video frames. This track can be referred to using the aliases `Default_Image` and `Image_1`.
- `taskName.Audio__1` (note the double underscore), an audio track, if audio is present in the stream from VMS. This track can be referred to using the alias `Default_Audio`.
- `taskName.Proxy` - the proxy track.

_FT_HTML5_bannerTitle.htm