Distributed Action Handler 12.12

# Configure SSL in a Unified System

Use the following procedure to configure SSL in a setup where you configure the DAH in the unified IDOL Server configuration file.

To configure an SSL connection in a unified system

1. Open the IDOL Server configuration file in a text editor.

2. Find the `[Server]` section, the `[IDOLServerN]` or `[DAHEngineN]` section, or a combination of the `[Server]` section and one of the others.

3. Add the `SSLConfig` setting to specify the section in which you have set the SSL details for the connection, usually `SSLOptionN`. For example:

       [Server]
       (other server settings...)
       SSLConfig=SSLOption0

       [IDOLServer0]
       SSLConfig=SSLOption0

       [IDOLServer1]
       SSLConfig=SSLOption1

   In this example, incoming ACI calls and outgoing calls to `IDOLServer0` share the same SSL configuration, and outgoing calls to `IDOLServer1` use a different configuration.

4. Create an `[SSLOptionN]` section for each unique `SSLConfig` setting. Each `SSLOption` entry must contain the `SSLMethod`, `SSLCertificate`, and `SSLPrivateKey` parameters. For example:

       [SSLOption0]
       SSLMethod=TLSV1.3
       SSLCertificate=host1.crt
       SSLPrivateKey=host1.key

       [SSLOption1]
       SSLMethod=TLSV1.3
       SSLCertificate=host2.crt
       SSLPrivateKey=host2.key

5. Save and close the configuration file. Restart the IDOL Server for your changes to take effect.

© Copyright 2022 Micro Focus or one of its affiliates
Version 12.12 | Last updated June 2022

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to swpdl.idoldocsfeedback@microfocus.com.

We appreciate your feedback!

Product: IDOL Distributed Action Handler 12.12

Topic Title: Configure SSL in a Unified System