Media Server 12.13

# BarcodeTypes

A comma-separated list of the types of barcodes that might appear in the ingested media. The following types are available:

Codabar Code-128 Code-39 Code-93 Datalogic 2/5 Data Matrix EAN-13 EAN-2 EAN-5 EAN-8 | I25 IATA 2/5 Industrial 2/5 Matrix 2/5 Patch Code PDF417 QR UPC-A UPC-E

NOTE: EAN-2 and EAN-5 supplement other barcodes (EAN-13, EAN-8, UPC-E, and UPC-A). Media Server does not read EAN-2 and EAN-5 barcodes unless they appear alongside one of these types. For example, to read EAN-13 barcodes that have an EAN-2 supplement, set `BarcodeTypes=EAN-13,EAN-2`.

NOTE: Some types of barcode are a subset of other types.

- UPC-A is a subset of EAN-13. If you configure Media Server to detect EAN-13 barcodes, Media Server returns all EAN-13 barcodes including UPC-A.
- ISBN barcodes are a subset of EAN-13 that begin with 978 or 979, so you can detect ISBN barcodes by configuring Media Server to detect EAN-13 barcodes, but Media Server will also return EAN-13 barcodes than are not in the ISBN range.
- GS1-128 barcodes (sometimes known as UCC/EAN-128) are a subset of Code-128 barcodes, so you can detect these using the Code-128 type.

Alternatively, you can set one of the following values to process multiple barcode types:

`All` | All supported types.
`All1D` | All one-dimensional types.
`All2D` | All two-dimensional types.

Type: | String (comma-separated list)
Default: | All
Required: | No
Configuration Section: | TaskName
Example: | `BarcodeTypes=QR`
See Also: |

© Copyright 2022 Micro Focus or one of its affiliates
Version 12.13 | Last updated October 2022

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to swpdl.idoldocsfeedback@microfocus.com.

We appreciate your feedback!

Product: IDOL Media Server 12.13

Topic Title: BarcodeTypes