Open topic with navigation

# MaxRemoteAnalysisConnections

The maximum number of requests, for remote analysis, to accept from other Media Servers simultaneously. This number includes requests that are being processed (the number of which is limited by RemoteAnalysisConfigurations) and the number that are queued.

A remote analysis task waits for a record to be processed and returned before sending another, so this is equivalent to the maximum number of remote analysis tasks that you should configure to send records to this Media Server.

Each connection requires an ACI thread, so ensure that you set the value of Threads to be greater than the value of this parameter.

Type: | Integer
Default: | 10
Required: | No
Configuration Section: | Chaining
Example: | `MaxRemoteAnalysisConnections=6`
See Also: | RemoteAnalysisConfigurations

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm