Open topic with navigation

# DAHEngine`N` Configuration

In the `[DAHEngines]` section you must create a `[DAHEngineN]` subsection for each IDOL server to which the Distributed Action Handler sends actions. Each `[DAHEngineN]` subsection specifies the host and ACI port of a child IDOL server. See Child Server Configuration Parameters.

NOTE:

You must number child IDOL server sections in consecutive order, starting from 0 (zero).

For example:

    [DAHEngines]
    Number=2

    [DAHEngine0]
    Host=localhost
    Port=9000

    [DAHEngine1]
    Host=12.3.4.56
    Port=9000

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm