Open topic with navigation

# AudioACIPort

The port that the Media Server audio service should use for receiving ACI actions. In most cases you can use the default value. You only need to set this parameter if the default port is already in use on your system.

Type: | Integer
Default: | The value of `[Server]` Port + 5
Required: | No
Configuration Section: | Resources
Example: | `AudioACIPort=14005`
See Also: |

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm