Open topic with navigation

# GPUBatchingDuration

NOTE:

This configuration parameter is available only if you have configured Media Server to use a GPU. For information about using a GPU to accelerate analysis, refer to the Media Server Administration Guide.

The maximum amount of time to wait before sending a batch of video frames to the GPU for analysis. After a video frame has been waiting in the queue for this amount of time, video frames are sent to the GPU even if the number of frames is less than that specified by GPUNumParallel.

To maximize throughput and use the GPU most efficiently, configure a long `GPUBatchingDuration` so that Media Server waits until there is a full batch of video frames to analyze. If you are processing low volumes of frames or require the analysis results as rapidly as possible, you can reduce the duration.

Type: | Time duration The value of this parameter is a time duration. Specify the duration in the following format:
         1days 2hours 3minutes 4seconds 500milliseconds 600microseconds
You can omit any of the individual durations when they are not required:
         4seconds 500milliseconds
You can also shorten the string by abbreviating the units to their first letter (milliseconds abbreviates to ms, microseconds to us):
         4s 500ms
The following are all equivalent:
         1minute 3seconds
         1m 3s
         63s
To specify an infinite duration, use the value `Infinite`.
Default: | 1000ms
Required: | No
Configuration Section: | TaskName
Example: | `GPUBatchingDuration=1500ms`
See Also: | GPUNumParallel

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm