# GUID

The Milestone GUID of the camera that the events should be associated with (the GUID of the camera that supplied the video). For information about finding the camera GUID, refer to the Milestone documentation.

You do not have to specify the camera GUID if you are ingesting video using the Milestone ingest engine. If you do not specify a GUID, Media Server automatically associates alarms to the camera that the Milestone ingest engine received the video from.

Type: | String
Default: |
Required: | Yes, unless you are ingesting video from Milestone using the Milestone ingest engine
Configuration Section: | TaskName
Example: |
See Also: |

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm