# MinRead

The minimum number of consecutive frames in which a number plate must be visible before a result is generated.

In most cases Micro Focus recommends that you use the default value. Reducing the value of this parameter could reduce accuracy.

Type: | Integer
Default: | 2
Required: | No
Configuration Section: | TaskName
Example: | `MinRead=5`
See Also: |

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm