# RequireGSSAuth

Set `RequireGSSAuth` to `True` to enable GSSAPI authentication mode on the Box Connector service port. In this mode, all connections to the service port must be authenticated using GSSAPI and the Negotiate HTTP authentication mechanism.

To use GSSAPI authentication, you must also set GSSServiceName, to define the GSSAPI service name that Box Connector must use to identify itself.

NOTE: This method provides an authentication requirement only. Micro Focus recommends that you use it in conjunction with TLS/SSL to encrypt the authentication data.

You cannot use `RequireGSSAuth` with GSS ACI encryption (see ACI Encryption Configuration Parameters). If you configure both, Box Connector does not start.

Type: | Boolean
Default: | False
Required: | No
Configuration Section: | Service
Example: | `RequireGSSAuth=True`
See Also: | GSSServiceName

© Copyright 2020 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm