# ClassificationServerPort

The ACI port to use to send actions to the IDOL Server Category component. Use this parameter when you are configuring the mailing operation to send channel results.

Type: | Long
Default: |
Allowed Range: | Minimum: 1 Maximum: 65535
Recommended Range: | Minimum: 1025 Maximum: 65535
Required: | No
Configuration Section: | `MyCustomFunctionality`
Example: | `ClassificationServerPort=1000`
See Also: | ClassificationServerHost ClassificationServerRetries ClassificationServerTimeout RunMailer

_FT_HTML5_bannerTitle.htm