Media Server 24.1

# Draw Regions

The `Draw` transformation task draws regions on images or video frames.

To draw regions on images and video frames

1. Create a new configuration to send to Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Session]` section, add a new task by setting the `EngineN` parameter. You can give the task any name, for example:

       [Session]
       Engine0=Ingest
       ...
       Engine2=Draw

3. Create a new configuration section to contain the task settings and set the following parameters:

   `Type` | The transformation engine to use. Set this parameter to `Draw`.
   `Input` | The name of the track that contains the images to draw on, with region data. The track must supply records that contain both an image and at least one region.
   `Color` | (Optional) The line color to use when drawing.
   `Thickness` | (Optional) The line thickness to use when drawing. Specify the thickness in pixels.

   For example:

       [Draw]
       Type=Draw
       Input=CombineESP.Output
       Color=Red
       Thickness=1

4. Save and close the configuration file. OpenText recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

Example configuration to ingest video and draw regions on encoded images

The following example configuration ingests a video file or stream and encodes one image for each detected face. Each image will show a red ellipse around the detected face.

    [Session]
    Engine0=Ingest
    Engine1=FaceDetect
    Engine2=Draw
    Engine3=Images

    [Ingest]
    Type=Video

    [FaceDetect]
    Type=FaceDetect
    NumParallel=6
    MinSize=10%

    [Draw]
    Type=Draw
    Input=FaceDetect.ResultWithSource
    Color=Red
    Thickness=2

    [Images]
    Type=ImageEncoder
    ImageInput=Draw.Output
    OutputPath=./output/%session.token%/%record.starttime.iso8601%.png

Example configuration to ingest video and draw regions on encoded video

The following example configuration ingests a video file or stream and encodes a video that shows detected faces by surrounding them with a red ellipse.

In this example, an ESP task combines the `Default_Image` track and the `FaceDetect.Data` track. This is necessary because the tracks produced by face detection only contain frames with detected faces, but to encode the video correctly we need to encode every frame.

    [Session]
    Engine0=Ingest
    Engine1=FaceDetect
    Engine2=Combine
    Engine3=Draw
    Engine4=MPEG

    [Ingest]
    Type=Video

    [FaceDetect]
    Type=FaceDetect
    NumParallel=6
    MinSize=10%

    [Combine]
    Type=Combine
    Input0=Default_Image
    Input1=FaceDetect.Data
    MaxTimeInterval=50ms

    [Draw]
    Type=Draw
    Input=Combine.Output
    Color=Red
    Thickness=2

    [MPEG]
    Type=mpeg
    VideoProfile=mpeg4video_h264_720p
    ImageInput=Draw.Output
    OutputPath=./output/%session.token%/%segment.startTime.iso8601%.ts

Copyright 2023 Open Text
Version 24.1 | Last updated December 2023

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Media Server 24.1

Topic Title: Draw Regions