Media Server 24.2

# Receive Ingest Engine

The Receive ingest engine ingests information (images or video frames, and metadata) that was output by another Media Server. For information about how to split processing across multiple Media Servers, refer to the Media Server Administration Guide.

To configure a task that uses the Receive ingest engine, you can set the following parameters:

Configuration Parameter | Description
--- | ---
Input | A comma-separated list of tracks to receive from the other Media Server.
Type | The type of ingest engine to use. Set this parameter to `Receive`.

The engine produces a track for each track specified by the `Input` parameter. For example, if you set `Input=FaceDetect.ResultWithSource`, the engine produces a track named `taskName.FaceDetect.ResultWithSource`, where `taskName` is the name of the Receive ingest task.

Copyright 2024 Open Text
Version 24.2 | Last updated March 2024

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Media Server 24.2

Topic Title: Receive Ingest Engine