Media Server 24.3

# Example Barcode Task Configuration

To detect and read barcodes, you could use the following task configuration:

    [Barcodes]
    Type=barcode
    BarcodeTypes=all
    Orientation=any

Setting the `BarcodeTypes` parameter to `all` detects all types of barcodes, including QR codes.

By default Media Server only detects barcodes that are upright, but setting the `Orientation` parameter to `any` means that Media Server can also detect barcodes that have been rotated by 90 or 180 degrees.

Copyright 2024 Open Text
Version 24.3 | Last updated June 2024

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Media Server 24.3

Topic Title: Example Barcode Task Configuration