Media Server 24.3

# Encoding

A configuration can contain any number of encoding tasks. For example:

    [Session]
    Engine0=Ingest
    Engine1=MyRollingBuffer

    [MyRollingBuffer]
    Type=rollingbuffer
    // rolling buffer configuration

This example specifies a single encoding task named `MyRollingBuffer`.

An encoding engine accepts image and/or audio tracks produced by an ingest or analysis engine. For example, you can:

- make a copy of ingested video.
- make a copy of ingested video at a different resolution or bitrate to the source.
- encode the output of an analysis engine - for example use the Image Encoder to write the keyframes identified by keyframe analysis to disk.

All encoding tasks produce a single output track with the name `TaskName.Proxy`, where `TaskName` is the name of the encoding task. This track contains information about the encoded media. You can output this information alongside your analysis results so that a front-end application can open and display the encoded media that shows a specific event, such as an identified news story or a recognized face.

Copyright 2024 Open Text
Version 24.3 | Last updated June 2024

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Media Server 24.3

Topic Title: Encoding