Media Server 24.3

# TimeBetweenAlarms

The minimum interval between alarms. This applies to all alarms. To specify no restriction, use the value 0.

Type: | Time duration The value of this parameter is a time duration. Specify a value using one or more of the following units:
         days          d
         hours         h
         minutes       m
         seconds       s
         milliseconds  ms
         microseconds  us
For example, all of the following are equivalent:
         1minute 3seconds
         1m 3s
         63s
Default: | 0 (no restriction)
Required: | No
Configuration Section: | TaskName
Example: | `TimeBetweenAlarms=2 seconds`
See Also: |

Copyright 2024 Open Text
Version 24.3 | Last updated June 2024

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Media Server 24.3

Topic Title: TimeBetweenAlarms