Community Component 25.1
Community Component Help

# ClassificationServerPort

The ACI port to use to send actions to the Category component. Use this parameter when you are configuring the mailing operation to send channel results.

Type: | Long
Default: |
Allowed Range: | Minimum: 1 Maximum: 65535
Recommended Range: | Minimum: 1025 Maximum: 65535
Required: | No
Configuration Section: | `MyCustomFunctionality`
Example: | `ClassificationServerPort=1000`
See Also: | ClassificationServerHost ClassificationServerRetries ClassificationServerTimeout RunMailer

Copyright 2024 Open Text
Version 25.1 | Last updated January 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Community Component 25.1

Topic Title: ClassificationServerPort