Distributed Action Handler 25.2
Distributed Action Handler Help

# DAH Engines Configuration Parameters

If you install and operate the DAH in a unified Knowledge Discovery configuration, you can configure child engines for DAH and DIH separately. This option allows you increased flexibility when querying and indexing content in remote servers. For example, you might define multiple DIH child engines for content that you index through a combination of failover and mirroring.

Use the `[DAHEngines]` section to set the total number of chlid servers to which the DAH sends actions.

You must create a `[DAHEngineN]` subsection for each child engines that DAH must send actions to. In this section, you specify the child server configuration details.

For example:

    [DAHEngines]
    Number=2

    [DAHEngine0]
    Host=localhost
    Port=9000

    [DAHEngine1]
    Host=12.3.4.56
    Port=9000

NOTE: This configuration for the DAH distribution child servers is not used for stand-alone DAH.

- For stand-alone configuration see Distributed Engine Configuration Parameters
- For unified configuration in which DAH and DIH are configured together, see Distribution IDOL Servers Configuration Parameters

Copyright 2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Distributed Action Handler 25.2

Topic Title: DAH Engines Configuration Parameters