Distributed Action Handler 25.2
Distributed Action Handler Help

# SSLConfig

Identifies the configuration section in which the SSL configuration details for distributed engines are specified, usually `SSLOptionN`. You must set this parameter if you are using SSL connections between DAH and child engines.

Setting this parameter in the `[Server]` section controls incoming ACI calls.

Setting this parameter in the `[DistributedEngineN]` section controls outgoing ACI calls to child engines in a Standalone DAH system.

Setting this parameter in the `[IDOLServerN]` section controls outgoing ACI calls to child engines in a DAH system that is integrated in a unified Knowledge Discovery configuration.

Setting this parameter in the `[DAHEngineN]` section controls outgoing ACI calls to child engines in a DAH system that is integrated in a unified Knowledge Discovery configuration in which DAH and DIH child engines are configured separately.

NOTE: You can set this parameter in the `[Server]` section alone, in `[DistributedEngineN]`, `[DAHEngineN]`, or `[IDOLServerN]` alone, or in both the `[Server]` and either `[DistributedEngineN]`, `[DAHEngineN]`, or `[IDOLServerN]` sections, depending on how you want to manage your connections.

If you create a server group by specifying a comma-separated list of host names in the Host parameter, you can use a single value for `SSLConfig` so that all child servers in the group use the same SSL details. Alternatively, you can use a comma-separated list to use different details for each mirrored child server. In this case, there must be the same number of values in `SSLConfig` as there are for Host.

Type: | String
Default: |
Required: | No
Configuration Section: | IDOLServer`N` or DistributedEngine`N` or DAHEngine`N`
Example: | `[DistributedEngine0] SSLConfig=SSLOption0` In this example, the SSL connection to DistributedEngine0 is configured in the SSLOption0 section. `... [Server] SSLConfig=SSLOption [DistributionIDOLServers] Number=2 [IDOLServer0] SSLConfig=SSLOption [IDOLServer1] SSLConfig=SSLOption1` In this example, incoming ACI calls and outgoing calls to IDOLServer0 use the same SSL configuration, but outgoing calls to IDOLServer1 use a different SSL configuration.
See Also: | Host Secure Socket Layer Parameters

Copyright 2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Distributed Action Handler 25.2

Topic Title: SSLConfig