Distributed Action Handler 25.2
Distributed Action Handler Help

# DAHEngine`N` Configuration

In the `[DAHEngines]` section you must create a `[DAHEngineN]` subsection for each child server to which the Distributed Action Handler sends actions. Each `[DAHEngineN]` subsection specifies the host and ACI port of a child server. See Child Server Configuration Parameters.

NOTE: You must number child server sections in consecutive order, starting from 0 (zero).

For example:

    [DAHEngines]
    Number=2

    [DAHEngine0]
    Host=localhost
    Port=9000

    [DAHEngine1]
    Host=12.3.4.56
    Port=9000

Copyright 2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Distributed Action Handler 25.2

Topic Title: DAHEngineN Configuration