# StartTimeout

The amount of time to wait to receive the first video frame from the XProtect recording server. If Media Server does not receive video, the connection times out.

Type: | Time duration The value of this parameter is a time duration. Specify the duration in the following format:
         1days 2hours 3minutes 4seconds 500milliseconds 600microseconds
You can omit any of the individual durations when they are not required:
         4seconds 500milliseconds
You can also shorten the string by abbreviating the units to their first letter (milliseconds abbreviates to ms, microseconds to us):
         4s 500ms
The following are all equivalent:
         1minute 3seconds
         1m 3s
         63s
Default: | 5 seconds
Required: | No
Configuration Section: | TaskName
Example: | `StartTimeout=3s`
See Also: |

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm