Media Server 24.1

# VideoSize

The size of the encoded video, in pixels (width followed by height).

To encode the video using the same dimensions as the video source, set this parameter to `copy`.

To maintain the aspect ratio of the source video, specify either a width or height and set the other dimension to zero, for example:

- `160x0` specifies a width of 160 and calculates the appropriate height using the original aspect ratio.
- `0x160` specifies a height of 160 and calculates the appropriate width using the original aspect ratio.

The following delimiters for the width and height are all acceptable: `160,90 160x90 160X90 160:90`.

Type: | List of integers
Default: | The size in the encoding profile, specified by VideoProfile
Required: | No
Configuration Section: | TaskName
Example: | `VideoSize=1920,1080`
See Also: | VideoProfile VideoBitrate

Copyright 2023 Open Text
Version 24.1 | Last updated December 2023

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Media Server 24.1

Topic Title: VideoSize